\documentclass[]{article}

%opening
\title{Instructions simple replay of Hall C Raster Data}
\author{}

\begin{document}

\maketitle

\begin{abstract}
Analysis of data taken with a spectrometer trigger to quickly see the raster pattern.
\end{abstract}
\section{ Description of Hall C raster system}

The Hall C raster system has two sets of XY rasters. For this document the rasters will be labeled: XA, YA, XB and YB. The voltage that drives the four fast rasters is 
put into the HMS and SHMS DAQ. For the HMS, the data is 
in ROC 11, slot 18, channels 12-15 for XA, YA, XB and YB. 
For the SHMS, the data is 
in ROC 2, slot 14, channels 12-15 for XA, YA, XB and YB.

\section{Analysis}
For a simple analysis of the raster data, the raster data is put into the TRIG apparatus  rather than the
standard raster detector class. The analysis can be done for HMS and/or SHMS data.   
\begin{itemize}
	\item Analysis is done in the hallc\_replay directory using hcana.
	\item Run either:
\begin{itemize}
		\item hcana SCRIPTS/HMS/replay\_hms\_raster\_simple(runnumber,-1)
		\item hcana SCRIPTS/SHMS/replay\_shms\_raster\_simple(runnumber,-1)
\end{itemize}
\item To look at histogram, cd to the onlineGUI directory
	\item Run either:
	\begin{itemize}
		\item ./online -f Config/HMS/RASTER/simple\_raster.cfg -r runnumber
		\item ./online -f Config/SHMS/RASTER/simple\_raster.cfg -r runnumber
	\end{itemize}
	\end{itemize}

	\end{document}
