Hall C User Howto

Run Monticello

Glen Warren April 7, 2003

Abstract This document describes how to run the MEDM screen monticello and how to access some of the most frequently used information.

1 Starting Monticello

To start Monticello, log in as either cvxwrks@cdaqh1 or cdaq@cdaqs3. Once connected, there are two ways to start:

1. from the window manager, left click on a blank part of the screen and select Monticello from the pop menu;

2. from the terminal, type runmonticello. The script is located in ~\bin\.

2 Accessing information

Below is a description of how to access some of the most often used screens from Monticello:

• CEBAF overview: Under the Comfort Screens drop-down menu button, choose “General CEBAF overview.”

• FSD overview: Click the FSD drop-down menu button, there is no menu.

• FSD for target movement: In the FSD overview screen, there is a box on the left side of the screen labeled “Target Movement Masking.” Click on the drop-down menu button and select “Mask Hall C Target Movement.”

• fast feedback: Click on the left drop-down menu button for Hall C, choose “Hall C Fast Feedback Control.”

• fast raster info: Under the left drop-down menu button for Hall C, choose “Hall C Raster, Fast.”

• Hall C overview: Click on the left drop-down menu button for Hall C, choose “Hall C General Info.”

• ion chambers: Click on the left drop-down menu button for RadCon, choose “Hall C Ion Chamber Signals.”

• polarized gun overview: Click on the left drop-down menu button for Gun/Laser, choose “PGun OPS Main.”

If anyone would like to add to this list, please contact the author.